关于 BarcodeScanner(&A)...

About Barcode Scanner(&A)…

与仪器建立连接失败

Communications fail…

从EEPROM读取参数失败

Read parameters from EEPROM fail…

当前仪器正在运行，不可再次运行

Scanner is working, no other operations…

当前仪器状态不正常，不可进行工作

Scanner in wrong work conditions, please recheck scanner…

当前仪器正在运行，不能退出软件

Scanner is working, please don’t quit software…

读取地址序号为%d的EEPROM参数出错

Read parameters from address % d EEPROM fail…

将EEPROM参数写入地址序号为%d时出错

Write EEPROM parameters into address % d EEPROM fail…

横向电机复位失败

X-axel motor reset fail

纵向电机复位失败

Y-axel motor reset fail

横向电机移动到包埋盒抽屉第%u行%u列位置失败

X-axel motor move to %u row & % u column fail

纵向电机移动到包埋盒抽屉第%u行%u列位置失败

Y-axel motor move to %u row & % u column fail

读取%u行%u列位置的条码信息失败

Read barcode information from % u row &%u column fail

横向电机脉冲输入不正确，请重新输入

X-axel motor pulse parameters are wrong, please re-input…

纵向电机脉冲输入不正确，请重新输入

Y-axel motor pulse parameters are wrong, please re-input…

横向电机正向移动指定脉冲失败

X-axel motor forward motion indication pulse is wrong…

横向电机反向移动指定脉冲失败

X-axel motor backward motion indication pulse is wrong…

横向电机移动到指定位置失败

X-axel motor move to designated spot is fail…

纵向电机正向移动指定脉冲失败

X-axel motor forward motion indication pulse is wrong…

纵向电机反向移动指定脉冲失败

Y-axel motor backward motion indication pulse is wrong…

纵向电机移动到指定位置失败

Y-axel motor move to designated spot is fail…

存在

Exist

不存在

No exist

读取条码信息失败

Read barcode information is fail…

仪器正在运行中，不能进行参数管理

Scanner is working; you can not setup parameters…

仪器正在运行中，不能进行系统检测

Scanner is working, you can not do system checking…

包埋盒抽屉未正确放置，请重新放置

Cassete drawer put into wrong Pos. please check it…

条码格式不匹配，扫描终止

Barcode format is not match to our scanner, scanning is terminated…

扫描结束

Scan job is done…